Call us

### +91 74001 6123

E-mail us

### info@darshanchemicals.in

### SAFETY

- Home
- SAFETY

### DESIGN SAFETY

- Fully ventilated plant
- 1.5 and 1.2 Mtr parallel staircases upto the top
- The plant is supported by 25 feet deep foundation resulting in very stable structure
- The plant has two gates and there are no obstacles for vehicles to enter from Gate NO1 and to exit from Gate No 2
- The plant is designed as per the norms of fire department of M.I.D.C and D.I.S.H

### PROCESS SAFETY

- All the vessel are equipped given pressure relief valves and rupture, discs
- All the vessels, receivers , tanks are provided with dip pipes to prevent Generation of Static charge.
- Auto temperature controllers are provided on each distillation system stopping inflow of thermic oil into system on achieving set temperature preventing unwanted rise in temperature.
- Other safety measures such as Copper Jumpers for Flanges, Flame Arrestors on vents & Nitrogen Anitisation are also taken.

### FIRE SAFETY

- 2280 LPM @75 meter head fire hydrant facility with mechanical foam spray
- 100,000 Ltr. underground water storage tank dedicated for fire fighting with slab load bearing capacity of 16 ton's.
- 10000 Ltr . overhead water tank kept at 100 feet height equipped with booster pump for firefighting purpose.
- We have sufficient no. of Fire extinguishers of different types such as ABC , DCP , MECHANICAL FOAM , CO2 , etc

### ELECTRICAL SAFETY

- All electrical equipments are flameproof
- Separate earth pits for plant , electrical panel , DG set , tanks , tankers loading , unloading and drum filling
- All the cable goes through cable trays

### Get in Touch

With decades of experience, we deliver consistent quality and
performance you can trust.

### Email us

info@darshanchemicals.in