Call us

### +91 74001 6123

E-mail us

### info@darshanchemicals.in

### Plant Details

- Home
- Plant Details

## PLANT DETAILS

Rec. No. | Capacity | PackedColumns Height / mtr. | Packing Type | Agitator | Condensors
--- | --- | --- | --- | --- | ---
R1 | 7.5 kl | 17 mtr | Sulzer Packings Wiregauge & Sheet Metal MOC-SS316L | Turbine | 45m2
R2 | 7.5 kl | 14 mtr | Anchor | 35m2
R3 | 5 kl | 14 mtr | Turbine | 45m2
R4 | 7.5 kl | 17 mtr | Anchor | 45m2
R5 | 1.2 kl | 8 mtr | Anchor | 25m2

### REACTOR DETAILS

- Various kettle sizes from 1.2 KL to 7.5 KL
- Specially designed Agitators to handle even highly viscous materials
- Stirrer rotation RPM up to 90 , ideal for fine crystallization
- All kettles have double mechanical seals for high temperature and high vacuum distillation.
- Double start limpet coils used for heating and cooling respectively
- MOC of all distillation reactors is SS316L

### COOLING DETAILS

- (300 TR) "Paharpur" make cooling tower
- The cooling tower is placed at 100 feet height
- Highly efficient cooling as the wind velocity at 100 feet height is more
- The pumping capacity required is less as the cooling tower is placed exactly above the condensers resulting in very less head required for pumping
- As the cooling tower placed above the condensers in case of power failure the condensers are filled with water from the cooling tower basin by gravity resulting in no vapor loss.
- Upto 45sq.mtr 4pass shell and tube type fully SS316L condensers and product coolers provide efficient cooling

### COLUMN DETAILS

- Meticulously designed columns can handle high vapor load at the same time provides high separation
- Column packed height up to 17 Mtr - Diameter up to 600 mm
- Suzler make wire gauge and sheet metal packing's with appropriate internals provide upto 65 Theoretical stages and very less pressure drop
- Separate 8 Mtr packed height column for high vacuum fractional distillation
- Tongue & groove flange in all column joints provides precise alignment and very less vacuum leakage.
- Temperature & pressure monitoring on all sections of column

### Material Storage Facility

### Warehouse

- Ample space for storage of filled and empty drums
- Fork lift facility for loading and unloading of drums

### Storage Facility

- 04 nos - 35 KL MS Storage tanks
- 02 nos - 20 KL MS Storage tanks

### Get in Touch

With decades of experience, we deliver consistent quality and
performance you can trust.

### Email us

info@darshanchemicals.in